DRAFT
IPMC INSPECTION CHECKLIST                                

BATHROOM

	
	Yes
	No
	Condition/Type
	Action
	Quantity

	502.1 Required facilities dwelling units -
Tub/shower, lavatory, water closet
Sanitary, safe working condition, location
	
	
	
	
	

	Tub/shower
504.1 Properly installed, no leaks or blockage
504.3 No hazards
505.3 Adequate water volume/pressure
505 Potable water, adequate hot/cold
506.1 Fixture connected to proper sanitary drainage
506.2 Stack, vent, waste and sewer functions properly and is free from leaks, obstructions and defects
	
	
	
	
	

	Lavatory
504.1 Properly installed, no leaks or blockage
504.3 No hazards
505.3 Adequate water volume/pressure
505 Potable water, adequate hot/cold
506.1 Fixture connected to proper sanitary drainage
506.2 Stack, vent, waste and sewer functions properly and is free from leaks, obstructions and defects
	
	
	
	
	

	Water closet
504.1 Properly installed, no leaks or blockage
504.3 No hazards
505.3 Adequate water volume/pressure
505 Potable water, adequate hot/cold
506.1 Fixture connected to proper sanitary drainage
506.2 Stack, vent, waste and sewer functions properly and is free from leaks, obstructions and defects
	
	
	
	
	

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Floors (walking surfaces)
Sound condition, good repair
404.2 Minimum room width 7 ft. (except kitchen)
Floor area =_______________

	
	
	
	
	

	402.1 and 403.1 Light and Ventilation
One window > or = 8% of floor area
Openable area 45% or more (of 8% floor area)
	
	
	
	
	

	403.2 Bathroom and Toilet Room Ventilation
Openable window or mechanical vent to outdoors
	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	BATHROOM (CONT)




	
	Yes
	No
	Condition/Type
	Action
	Quantity

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	602 Heating facilities
Capable of maintaining 68°F
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Correct all hazards
	
	
	
	
	

	605.2 Receptacle
At least one receptacle present
(new receptacles must be GFCI)
	
	
	
	
	

	605.3 Lighting fixtures
At least one is present
	
	
	
	
	






















IPMC INSPECTION CHECKLIST
BEDROOM

	
	Yes
	No
	Condition/Type
	Action
	Quantity

	404.1 Privacy
404.4.2 Access from bedrooms
Access or egress not through bedroom
404.4.3 Water closet accessibility
	
	
	
	
	

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Floors (walking surfaces)
Sound condition, good repair
404.2 Minimum room width 7 ft. (except kitchen)
Floor area =_______________

	
	
	
	
	

	404.4.1 Area for sleeping
Occupancy – 1 person/70 SF
More than 1 person /50 SF each
Allowed occupancy (circle one)
    1 person
    2 people
    3 people
	
	
	
	
	

	402.1 and 403.1 Light and Ventilation
One window > or = 8% of floor area
Openable area 45% or more (of 8% floor area)
	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	Doors
305.4 Good, clean, sanitary, no unsound paint
305.6 Interior door, well-fit, openable/closeable, securely attached
	
	
	
	
	

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	602 Heating facilities
Capable of maintaining 68°F
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards


	
	
	
	
	

	BEDROOM (CONT)



	
	Yes
	No
	Condition/Type
	Action
	Quantity

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe 
604.3 Electrical systems hazards
Correct all hazards
	
	
	
	
	

	704.2 Smoke alarms
1) One approved alarm is located in the sleeping room, and
2) Another alarm is located outside the room in the immediate vicinity
3) Alarms are located on each story within the unit including the basement
	
	
	
	
	




































IPMC INSPECTION CHECKLIST
DINING ROOM                                              
	
	Yes
	No
	Condition/Type
	Action
	Quantity

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Floors (walking surfaces)
Sound condition, good repair
404.2 Minimum room width 7 ft. (except kitchen)
Floor area =_______________

	
	
	
	
	

	404.5 Overcrowding
Required dining room –
80 SF - 3-5 occupants
150 SF - 6 or more occupants
Is living room occupancy sufficient for total bedroom occupancy and dining room occupancy?
(If no, unit is overcrowded and ineligible for assistance without resolution)
	
	
	
	
	

	402.1 and 403.1 Light and Ventilation
One window > or = 8% of floor area
Openable area 45% or more (of 8% floor area)
	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	Doors
305.4 Good, clean, sanitary, no unsound paint
305.6 Interior door, well-fit, openable/closeable, securely attached
	
	
	
	
	

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	602 Heating facilities
Capable of maintaining 68°F
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	



IPMC INSPECTION CHECKLIST

EXTERIOR PROPERTY AREAS

	
	Yes
	No
	Condition/Type
	Action
	Quantity

	302.1 Sanitation
Clean and free from rubbish and garbage
	
	
	
	
	

	302.2 Grading and Drainage
Erosion of soil, ponding/stagnant water, water within structure
	
	
	
	
	

	302.3 Sidewalks and Driveways
Proper repair, free from hazards (tripping, ice ponding)
	
	
	
	
	

	302.4 Weeds
Noxious weeds, growth height
	
	
	
	
	

	302.5 Rodents
Evidence of presence?
Harborage?
· Weeds
· Rubbish
· Garbage
Inoperable cars
	
	
	
	
	

	302.6 Exhaust vents
Hazardous discharge/noise
	
	
	
	
	

	302.7 Accessory structures
Structurally sound/ good repair
Structure type
· Garage
· Fence
· Wall
Other_______________

	
	
	
	
	

	302.7 Motor vehicles
· Inoperable
· Unlicensed
	
	
	
	
	

	302.8 Defacement of property
Location__________________

	
	
	
	
	

	303.1 Pools, Spas and Hot Tubs
Clean, sanitary, in good repair
	
	
	
	
	

	303.1 Enclosure
Depth of water > 24”?
Barrier height at least 48”?
Self latching gate?
	
	
	
	
	

	307.1 Accumulation of Rubbish/
Garbage
Free of
	
	
	
	
	

	307.2  and 307.3 Disposal of
Rubbish/Garbage
Approved containers
307.2.1 With covers
307.3.1 Garbage facilities
Approved grinder, incinerator or leak proof covered container
	
	
	
	
	

	507.1 Storm drainage
No nuisance created
	
	
	
	
	

	604.1 Electrical facilities
Required occupied dwelling unit is provided with three wire service of at least 60 amps in compliance with ICC Electrical Code
	
	
	
	
	

	604.3 Electrical systems hazards
Correct all hazards

	
	
	
	
	

	EXTERIOR PROPERTY AREAS (CONT)



	
	Yes
	No
	Condition/Type
	Action
	Quantity

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	






















































IPMC INSPECTION CHECKLIST
EXTERIOR STRUCTURE
	
	Yes
	No
	Condition
	Action
	Quantity

	304.1 General
Good repair, structurally sound, sanitary
	
	
	
	
	

	304.2 Protective treatment (Paint)
Is it pre 1978?  
If yes, order risk assessment
	
	
	
	
	

	304.3   Premises identification
(address numbers)
	
	
	
	
	

	304.4    Structural members
Free from deterioration and capable of support
	
	
	
	
	

	304.5    Foundation walls
Plumb, free from cracks, no rodent entry
	
	
	
	
	

	304.6    Exterior walls
Sound, weatherproof, coated
       Square feet ___________

	
	
	
	
	

	304.7    Roofs and Flashing

	
	
	
	
	

	304.7   Roof drainage
Gutters, downspouts, drains
	
	
	
	
	

	304.8    Decorative features
304.9    Overhand extensions
Good repair, safe, anchored, coated
	
	
	
	
	

	304.10 Chimneys and Towers
Safe, sound, good repair, coated
	
	
	
	
	

	304.13 Windows
Sound, good repair, weather tight
303.13.1 Glazing free of cracks and holes
303.13.2 Openable and hold open hardware
304.14 Insect screens
304.18.2 Sash locking device within 6 feet of ground
	
	
	
	
	

	304.15    Doors
Good condition, locks, security, egress (§702.3)
304.13  Door frames Sound, good repair, weather tight
304.18 Security
304.18.1 Egress
	
	
	
	
	

	304.16    Basement hatchways
Prevents entrance of rodents, rain and drainage water
304.18.3  Security
	
	
	
	
	

	304.10  Stairways
Structurally sound, good repair
304.12 Handrails and guardrails
Firm, good condition
306.1 Handrails and guardrails
With 4+risers
	
	
	
	
	

	304.10    Decks, Porches and Balconies
Structurally sound, good repair
304.12 Handrails and guardrails
Firm, good condition
306.1 Handrails and guardrails >30 inches in height
	
	
	
	
	

	304.17  Guards for basement windows
Rodent shields
	
	
	
	
	

	506 Sanitary drainage
All fixtures connected to approved disposal
506.2 Properly maintained
	
	
	
	
	

	EXTERIOR STRUCTURE (CONT)



	
	Yes
	No
	Condition/Type
	Action
	Quantity

	604.1 Electrical facilities
Required occupied dwelling unit is provided with three wire service of at least 60 amps in compliance with ICC Electrical Code
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Correct all hazards
	
	
	
	
	







































IPMC INSPECTION CHECKLIST

FURNACE/WATER HEATER ROOM


	
	Yes
	No
	Condition/Type
	Action
	Quantity

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Correct all hazards
	
	
	
	
	

	605.3 Lighting fixtures
At least one present
	
	
	
	
	

	603.1 Mechanical appliances
Properly installed, safe working condition, capable of performing as intended
603.2 Fuel burners connected to approved chimney or vent
603.3 Required clearance from combustibles is maintained
603.4 Safety controls in effective operation
	
	
	
	
	

	603.5 Combustion air
Is supplied for combustion of fuel and ventilation of space containing fuel burning equipment
	
	
	
	
	

	603.6 Energy conservation devices
Attached to fuel supply or vent and are labeled and properly approved
	
	
	
	
	

	607.1 Duct systems
Free of obstructions and capable of performing required functions
	
	
	
	
	

	703.1 Fire resistance-rated assemblies
Shall be maintained
	
	
	
	
	




















IPMC INSPECTION CHECKLIST

HABITABLE ROOMS INTERIOR STRUCTURE

	
	Yes
	No
	Condition/Type
	Action
	Quantity

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Floors (walking surfaces)
Sound condition, good repair
404.2 Minimum room width 7 ft. (except kitchen)
Floor area =_______________

	
	
	
	
	

	402.1 and 403.1 Light and Ventilation
One window >8% of floor area
Openable area 45% or more (of 8% floor area)
	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	Doors
305.4 Good, clean, sanitary, no unsound paint
305.6 Interior door, well-fit, openable/closeable, securely attached
	
	
	
	
	

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	








IPMC INSPECTION CHECKLIST

KITCHEN

	
	Yes
	No
	Condition/Type
	Action
	Quantity

	404.2 Minimum width
3 ft. between counter fronts/appliances/walls
	
	
	
	
	

	404.7 Food preparation
Suitable space and equipment to store, prepare and serve foods; sanitary disposal and temporary storage
	
	
	
	
	

	502.1 Required facilities dwelling units -
Kitchen sink
Sanitary, safe working condition
504.1 Properly installed, no leaks or blockage
504.3 No hazards
505.3 Adequate water volume/pressure
505 Potable water, adequate hot/cold
506.1 Fixture connected to proper sanitary drainage
506.2 Stack, vent, waste and sewer functions properly and is free from leaks, obstructions and defects
	
	
	
	
	

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Floors (walking surfaces)
Sound condition, good repair
404.2 Minimum room width 7 ft. (except kitchen)
Floor area =_______________

	
	
	
	
	

	402.1 and 403.1 Light and Ventilation
One window > or = 8% of floor area
Openable area 45% or more (of 8% floor area)
	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	Doors
305.4 Good, clean, sanitary, no unsound paint
305.6 Interior door, well-fit, openable/closeable, securely attached
	
	
	
	
	

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	
KITCHEN (CONT)


	
	Yes
	No
	Condition/Type
	Action
	Quantity

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	602 Heating facilities
Capable of maintaining 68°F
	
	
	
	
	

	603.1 Cooking appliance (stove)
Properly installed, safe and performs intended function
603.3 Clearance from combustible material
603.4 Safety controls in effective operation
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.3 Lighting fixtures
At least one is present
	
	
	
	
	




























IPMC INSPECTION CHECKLIST
LAUNDRY ROOM

	
	Yes
	No
	Condition/Type
	Action
	Quantity

	Clothes Washer
603.1 Mechanical appliances
Properly installed, safe working condition
504.1 Properly installed, no leaks or blockage
504.3 No hazards
505.3 Adequate water volume/pressure
505 Adequate hot/cold
506.1 Fixture connected to proper sanitary drainage
506.2 Stack, vent, waste and sewer functions properly and is free from leaks, obstructions and defects
	
	
	
	
	

	Laundry Sink
504.1 Properly installed, no leaks or blockage
504.3 No hazards
505.3 Adequate water volume/pressure
505 Adequate hot/cold
506.1 Fixture connected to proper sanitary drainage
506.2 Stack, vent, waste and sewer functions properly and is free from leaks, obstructions and defects
	
	
	
	
	

	Clothes dryer exhaust
Independent and correctly exhausted
603.1 Mechanical appliances properly installed, safe working condition
603.2 If gas, removal of combustion products and 603.5 combustion air
	
	
	
	
	

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Floors (walking surfaces)
Sound condition, good repair
404.2 Minimum room width 7 ft. (except kitchen)
Floor area =_______________

	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	Doors
305.4 Good, clean, sanitary, no unsound paint
305.6 Interior door, well-fit, openable/closeable, securely attached
	
	
	
	
	

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	
LAUNDRY ROOM (CONT)


	
	Yes
	No
	Condition/Type
	Action
	Quantity

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.2 Receptacle
Contains at least one grounded receptacle or GFCI
	
	
	
	
	

	605.3 Lighting fixture
At least one is present
	
	
	
	
	





























IPMC CHECKLIST – LIVING ROOM
                                              
	
	Yes
	No
	Condition/Type
	Action
	Quantity

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Floors (walking surfaces)
Sound condition, good repair
404.2 Minimum room width 7 ft. (except kitchen)
Floor area =_______________

	
	
	
	
	

	404.5 Overcrowding
Required living room –
120 SF - 3-5 occupants
150 SF - 6 or more occupants
Is living room occupancy sufficient for total bedroom occupancy and dining room occupancy?
(If no, unit is overcrowded and ineligible for assistance without resolution)
	
	
	
	
	

	402.1 and 403.1 Light and Ventilation
One window > or = 8% of floor area
Openable area 45% or more (of 8% floor area)
	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	Doors
305.4 Good, clean, sanitary, no unsound paint
305.6 Interior door, well-fit, openable/closeable, securely attached
	
	
	
	
	

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	602 Heating facilities
Capable of maintaining 68°F
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	



IPMC INSPECTION CHECKLIST

INTERIOR STAIRWAY

	
	Yes
	No
	Condition/Type
	Action
	Quantity

	305.1 General
Interior and equipment in good repair, structurally sound, sanitary
	
	
	
	
	

	305.2 Structural Members
Structurally sound/capable
	
	
	
	
	

	305.4 Stairs and walking surfaces
Sound condition, good repair
	
	
	
	
	

	305.5 Handrails and guardrails
Firmly fastened
306.1 Capable of loads, good condition Required 4+ risers or 30+ inches
	
	
	
	
	

	402.2/3 Light
Sufficient to permit safe utilization
	
	
	
	
	

	404.3 Minimum ceiling height
Not less than 7 ft. (with exceptions)
	
	
	
	
	

	308.1 Infestation
Free from insects and rodents
	
	
	
	
	

	Doors
305.4 Good, clean, sanitary, no unsound paint
305.6 Interior door, well-fit, openable/closeable, securely attached
	
	
	
	
	

	Windows
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or defective surface conditions
	
	
	
	
	

	Walls
305.3 Interior surfaces maintained in good sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Ceiling
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint, cracked or loose plaster or defective surface conditions
	
	
	
	
	

	Woodwork
305.3 Interior surfaces maintained in good, sanitary condition, no deteriorated paint or decay in wood or other defective surface conditions
	
	
	
	
	

	604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.1 Electrical equipment installation
All equipment, wiring, appliances properly installed and safe
604.3 Electrical system hazards
Correct all hazards
	
	
	
	
	

	605.3 Lighting fixtures
At least one is present
	
	
	
	
	








IPMC INSPECTION CHECKLIST

Other Locations (yet to be developed)

Basement

Crawlspace

Attic space

COMMUNITY REVITALIZATION TRAINING CENTER
