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	INTERIOR DECORATION  WORKS FOR UNITED INDIA  INSURANCE CO. LTD.
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	8th FLOOR , KANCHANJUNGA BUILDING , 18 BARAKHAMBA ROAD, NEW DELHI-110001.
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	BRANCH OFFICE AT UDYOG NAGAR METRO STATION , NEW DELHI.
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	ID WORKS
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	S NO
	
	ITEM / WORKS
	SUB
	SPECIFICATIONS
	UNITS
	
	QTY
	RATES IN
	RATES IN FIGURES
	AMOUNT
	TOTAL

	
	
	
	HEAD
	
	
	
	
	WORDS
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	A
	
	
	CIVIL WORK
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	DISMANTLING
	
	
	
	
	
	
	
	
	

	
	
	
	WORK
	
	
	
	
	
	
	
	
	

	
	I
	
	Disposal of malba
	
	
	LS
	
	3.00
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	TOTAL COST OF
	
	
	
	
	
	
	
	
	

	
	
	
	THE WORKS
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	PROPOSED CIVIL
	
	
	
	
	
	
	
	
	

	B
	
	
	CONSTRUCTIVE
	
	
	
	
	
	
	
	
	

	
	
	
	WORKS
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	CIVIL WORK
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	Providing & laying 75mm thick cement concrete
	
	
	
	
	
	
	

	
	
	
	
	
	flooring (IPS) in 1:2:4 (1 cement :2 coarse sand: 4
	
	
	
	
	
	
	

	
	
	
	Flooring ( Cement
	
	graded stone aggrgate 20mm nominal size) finished
	
	
	
	
	
	
	

	
	I
	
	
	i
	with floating coat of neat cement including cement
	CMT
	
	1.00
	
	
	
	

	
	
	
	Concrete)
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	slurry, rounding off edges laid in alternate bays ,
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	including mixing of the cement admixture to enhance
	
	
	
	
	
	
	

	
	
	
	
	
	the impervious quality of the cc. complete
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	II
	
	Plaster
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	P / A 12mm thick plaster in cement mortar 1 :4 to  all
	
	
	
	
	
	
	

	
	
	
	
	
	types of  RCC / brick work, columns, surfaces including
	
	
	
	
	
	
	

	
	b
	
	1:4 Cement Mortar
	
	wall  tops, jambs and sills etc.  in line level and  plumb,
	SMT
	
	2.00
	
	
	
	

	
	
	
	
	
	including smooth cement finish, including providing
	
	
	
	
	
	
	

	
	
	
	
	
	necessary  grooves, if required
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	TOTAL COST OF
	
	
	
	
	
	
	
	
	

	
	
	
	THE WORKS
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	C
	
	
	FLOORING
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	P / L First class 600 x 600mm vitrified tiles brand asian
	
	
	
	
	
	

	
	
	
	
	granito model Morocco using 1:4 cement mortar in
	
	
	
	
	
	

	
	
	
	
	floor & 100mm high dado, with machine cutting as
	
	
	
	
	
	

	
	
	
	
	required, gaps treated with grout with an admixture of
	
	
	
	
	
	

	
	
	
	
	pigment to match the shade of tile and joints to match
	
	
	
	
	
	

	
	
	
	
	the ones on floor and with dado, as per drawing and
	
	
	
	
	
	

	
	I
	Vitrified Tile Flooring
	i
	specifications including providing & APPLYING POP
	SMT
	85.00
	
	
	
	

	
	
	
	
	ON FLOORING FOR FLOOR PROTECTION WITH
	
	
	
	
	
	

	
	
	
	
	PLASTIC SHEET OF 150 TO 200 MICRONS
	
	
	
	
	
	

	
	
	
	
	THK.BETWEEN THE FLOORING AND POP. THE
	
	
	
	
	
	

	
	
	
	
	RATE MUST INCLUDE THE CLEANING OF THE POP
	
	
	
	
	
	

	
	
	
	
	AND PLASTIC ON COMPLETION OF OTHER
	
	
	
	
	
	

	
	
	
	
	WORKS TO EXPOSE THE FLOORING etc.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	TOTAL COST OF
	
	
	
	
	
	
	
	

	
	
	THE WORKS
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	E
	
	FALSE CEILING
	
	
	
	
	
	
	
	

	
	
	WORKS
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	P/Fixing of Mineral fiber ceiling system with mineral
	
	
	
	
	
	

	
	
	
	
	fibre tiles  having a life long guarantee with Humidity
	
	
	
	
	
	

	
	
	
	
	resistance of 95%, NRC of 0.55- 0.6,Sound
	
	
	
	
	
	

	
	I
	T GRID CEILLING
	
	Attenuation -34db,in module of size of 600mm
	SMT
	80.00
	
	
	
	

	
	
	ARMSTRONG
	
	x600mm x15mm,micro look edges to be laid on
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Silouhette Grid.. The cost would  include cost for
	
	
	
	
	
	

	
	
	
	
	suspenders, dash-fasterners, associated hardware,
	
	
	
	
	
	

	
	
	
	
	cutting for lights & speakers in the ceiling tile).
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	II
	POP PUNNING ON
	
	
	SMT
	15.00
	
	
	
	

	
	
	WALL
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	TOTAL COST OF
	
	
	
	
	
	
	
	

	
	
	THE WORKS
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	G
	
	DOOR WORKS
	
	Note 1: All doors to include door acccessories- Door
	
	
	
	
	
	

	
	
	(Shutter )
	
	closer, door handle, door lock, and door buffer.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Note 2: All the floor springs/ door closers to be Used
	
	
	
	
	
	

	
	
	
	
	from Dorset make. Door closer/ floor spring to be
	
	
	
	
	
	

	
	
	
	
	selected as per the weight of the door, as specified by
	
	
	
	
	
	

	
	
	
	
	the manufacturer.
	
	
	
	
	
	

	
	
	
	
	Note 3: All door Handles  and mortic Locks to be from
	
	
	
	
	
	

	
	
	
	
	Dorset or Ozone. Door Handle for toughened glass
	
	
	
	
	
	

	
	
	
	
	doors- SD 10 P SS- 12" long handle SS Handle from
	
	
	
	
	
	

	
	
	
	
	Dorset.  All patch fittings to be from Ozone make.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Note 4: All hinges being used to be in SS and all
	
	
	
	
	
	

	
	
	
	
	hinges to be Ball Bearing hinges , Hinges (4") to be
	
	
	
	
	
	

	
	
	
	
	used per door.
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TOTAL



Note 5: All door chowkhats to be in first class Steem

beach, unless specified otherwise.

	
	Glazed Door shutter
	Providing and fixing Glass door ( 6 mm thick) with
	
	

	
	including harware and
	
	
	

	I
	
	Lower Stile of  8" and upper stile of 5" complete
	SMT
	5.80

	
	door closures and
	
	
	

	
	
	inclusive all fixing accessories and all incidentals.
	
	

	
	fittings
	
	
	

	
	
	
	
	

	
	
	Providing & fixing double shutter TOUGHENED  Glass
	
	

	
	
	doors of size as per drawing fabricated with 12mm thk
	
	

	
	
	TOUGHENED glass (Modi Guard / Saint Gobain),with
	
	

	
	
	approved patch fittings as shown in the standard
	
	

	
	
	detailed drawing & floor springs. It shall have approved
	
	

	II
	Front Glass Shutter
	stainless steel door handles on both sides and suitable
	SMT
	7.00

	
	
	locking arrangement etc. all as directed &to the entire
	
	

	
	
	satisfaction of Architect / owner.
	
	

	
	
	All the fittings shall be of Ozone make, Handle of Neki
	
	

	
	
	make - H shape (25mm dia - 2' long)
	
	

	
	
	
	
	

	III
	Architrave Moulding
	Providing and fixing Architrave Moulding
	RMT
	31.00

	
	
	
	
	

	IV
	Door Frames
	Providind and Fixing  Woodwork in Chowkhats  Steem
	RMT
	15.70

	
	
	Beech wood unless specified.
	
	

	
	
	
	
	

	
	
	
	
	

	
	TOTAL COST OF
	
	
	

	
	THE WORKS
	
	
	

	
	
	
	
	

	
	PARTITION AND
	Note 1: All the wooden members/ boards/ panels being
	
	

	I
	
	used will have to be given anti-termite ( with 5 years
	
	

	
	PANELLING  WORKS
	
	
	

	
	
	guarantee) and fire retardant treatment at site.
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	Note 2: All the laminates to be used from "Woodgrain"
	
	

	
	
	series from Merino lam  or equivalent from Century/
	
	

	
	
	Greenlam/ Royal Touch, min. 1mm thk conforming to
	
	

	
	
	IS 2217.
	
	

	
	
	
	
	

	
	
	Note 3: All the glass to be float glass (unless specified
	
	

	
	
	otherwise) from ASAHI / SAINT GOBAIN. All patch
	
	

	
	
	fittings to be from Ozone make.
	
	

	
	
	
	
	

	
	
	Note 4: All Gypsum Board (MR Grade) and GI sections
	
	

	
	
	to be of Gypsum India make.
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	P/F glazed partition with following details: .both side
	
	
	
	
	
	

	
	
	FULL HEIGHT HALF
	
	12mm th. comm. ply, Bottom to have laminated skirting
	
	
	
	
	
	

	
	
	
	
	of approx. 100mm width. complete as per detailed
	
	
	
	
	
	

	
	i
	TRANSPARENT
	
	
	SMT
	45.00
	
	
	
	

	
	
	
	
	dwgs. Note (1) cost not to include the polishing/
	
	
	
	
	
	

	
	
	PARTITION
	
	
	
	
	
	
	
	

	
	
	
	
	staining  of wood as per approved sample , (2) Cost to
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	include float glass of 6mm thk.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	LOW HEIGHT
	
	
	
	
	
	
	
	

	
	ii
	PARTITION WITH
	
	Top rail 3"X1" steam beach wood
	SMT
	20.00
	
	
	
	

	
	
	TOP RAIL
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	iii
	WALL PANELLING
	
	P/F with wooden frame and 12mm th. Ply
	SMT
	4.00
	
	
	
	

	
	
	WORK
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	GLASS FOR  LOW
	
	Providing & laying 12mm TOUGHENED GLASS
	
	
	
	
	
	

	
	iv
	
	
	EDGE POLISHING ALL SIDE FIXING WITH SS
	SMT
	2.00
	
	
	
	

	
	
	HEIGHT PARTITION
	
	
	
	
	
	
	
	

	
	
	
	
	CLAMP.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	TOTAL COST OF
	
	
	
	
	
	
	
	

	
	
	THE WORKS
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	J
	
	PAINT AND
	
	
	
	
	
	
	
	

	
	
	POLISHING
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Providing and applying plastic emulsion of approved
	
	
	
	
	
	

	
	
	
	
	colour & shade, cleaning the surface and make it free
	
	
	
	
	
	

	
	
	
	
	from dust by scrapping, cleaning etc., including
	
	
	
	
	
	

	
	
	
	
	application of two coats acrylic putty of approved make
	
	
	
	
	
	

	
	
	
	
	over the walls and ceiling to make it the same in line
	
	
	
	
	
	

	
	
	
	
	and level; application of primer coat over the same;
	
	
	
	
	
	

	
	I
	Plastic Emulsion
	
	application of minimum two or more coats of plastic
	SMT
	180.00
	
	
	
	

	
	
	
	
	emulsion of Asian paints / ICI Paints  or equivalent upto
	
	
	
	
	
	

	
	
	
	
	the desired finish of the EIC and protecting till the
	
	
	
	
	
	

	
	
	
	
	handing over of site including required scafolding,
	
	
	
	
	
	

	
	
	
	
	cleaning, filling up cracks with approved crack filler etc.
	
	
	
	
	
	

	
	
	
	
	all complete at all levels and leads to entire satisfaction
	
	
	
	
	
	

	
	
	
	
	of the Architect/Owner.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	II
	MELAMINE POLISH
	
	Providing and appliying polish wih melamine coating on
	SMT
	9.00
	
	
	
	

	
	
	
	
	all exposed wood
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	TOTAL COST OF
	
	
	
	
	
	
	
	

	
	
	THE WORKS
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	S NO
	ITEM / WORKS
	SUB
	
	SPECIFICATIONS
	UNITS
	QTY
	RATES IN
	RATES IN FIGURES
	AMOUNT
	TOTAL

	
	
	HEAD
	
	
	
	
	WORDS
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	H
	
	FURNITURE WORKS
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	3
	TABLE
	
	Scope : Providing , Manufacturing, Fixing in
	
	
	
	
	
	

	
	
	
	
	Position
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	The top : 19 mm thk Commercial board with 1.0
	
	
	
	
	
	

	
	
	
	
	mm laminate in the pattern approved. The top
	
	
	
	
	
	

	
	
	
	
	with TW Cornice moulding 2 1/4" x 1 1/2" all
	
	
	
	
	
	

	
	
	
	
	arround.
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Facia: 19 mm thk Commercial board with 1.0 mm
	
	
	
	
	
	

	
	
	
	
	laminate
	top in the pattern approved.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Structure paint :with fire paint of Vampire or
	
	
	
	
	
	

	
	
	
	
	equivalent
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Finishes: The Steam beech wooden surfaces to
	
	
	
	
	
	

	
	
	
	
	be melamnine polished.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	a
	MGR
	
	Size: 7'0"
	x 3'0" with side unit 3' x 18"
	NOS
	1.00
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	b
	ASST/MGR
	
	Size: 5'0"
	x 2'0" with side unit 3' x 18"
	NOS
	2.00
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	5
	LOW HEIGHT
	
	
	
	SMT
	6.00
	
	
	
	

	
	
	CABINET
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Scope : Providing , Manufacturing, Fixing in
	
	
	
	
	
	

	
	
	
	
	Position
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Height: 30" high
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Depth : 18"
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	The top : 25 mm thk Post formed top Bull
	
	
	
	
	
	

	
	
	
	
	Nose/edge taping
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Front Shutter: 19 mm thk Post formed top , edge
	
	
	
	
	
	

	
	
	
	
	taping
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	The Box Structure: 19 mm thk PLPB of approved
	
	
	
	
	
	

	
	
	
	
	laminate shade.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Fixing : Fixed to the exsiting Partition with
	
	
	
	
	
	

	
	
	
	
	Fasteners and Gitti
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Other: Includes all hardware for fixing in plumb
	
	
	
	
	
	

	
	
	
	
	line, Adhesive of Pidilite, including Hardware - 3"
	
	
	
	
	
	

	
	
	
	
	to 4" SS handles of approved design, self closing
	
	
	
	
	
	

	
	
	
	
	0 to 8 crenk hinges, Ball catcher, Chitakni, and
	
	
	
	
	
	

	
	
	
	
	Lock by Godrej.
	
	
	
	
	
	

	
	
	
	
	Method of meaurement: Front side
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	S NO
	ITEM / WORKS
	SUB
	SPECIFICATIONS
	UNITS
	QTY
	RATES IN
	RATES IN FIGURES
	AMOUNT
	TOTAL

	
	
	HEAD
	
	
	
	WORDS
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Providing and fixing in position 25mm thk Postformed
	
	
	
	
	
	

	
	
	
	
	working table of approved laminate finish. Including
	
	
	
	
	
	

	
	6
	Post form Work top
	
	Manufacturing /Providing / Fixing Top & structure made
	SFT
	63
	
	
	
	

	
	
	
	
	of 19mm thk prelam board edge binded.as per drawing
	
	
	
	
	
	

	
	
	
	
	etc
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	Cabinets having full laminated PLPB shutters 3/4"
	
	
	
	
	
	

	
	
	
	
	thick, with drawer units and a shutter unit out of 3.4"
	
	
	
	
	
	

	
	
	
	
	thick PLB @1'4" -1'6" ht (refer drawing), with shutters
	
	
	
	
	
	

	
	7
	Pedestal Units
	
	out of postformed PLPB panels, top to be out of
	NOS
	7
	
	
	
	

	
	
	
	
	postformed PLPB 19 mm, the sides to be 3/4" PLPB,
	
	
	
	
	
	

	
	
	
	
	laminated with edge lipping, complete as per drawing,
	
	
	
	
	
	

	
	
	
	
	2'6 " ' high, 1' 8" deep.
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	8
	Key board ms powder
	
	
	NOS
	12
	
	
	
	

	
	
	coating
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	TOTAL COST OF
	
	
	
	
	
	
	
	

	
	
	THE WORKS
	
	
	
	
	
	
	
	

	
	
	TOTAL OF ALL
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	THE  WORKS
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