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Inspection Checklist For Rental Properties

City Of West Lafayette, IN

Date:

Inspector Name:
Property address:
Type of Property:
Time In:	Time Out:


Electrical Panel:

[image: ][image: ]Service amps adequate for usage

[image: ][image: ]Properly grounded and in good condition

[image: ][image: ]No open circuits in box

[image: ][image: ]If fuses – proper sizes

[image: ][image: ]Adequate clearance and easy access

[image: ][image: ] All equipment installed and maintained to code

__________________________________
__________________________________

__________________________________
General Electrical:
[image: ][image: ]Covers on switches & outlets

[image: ][image: ]Splices to code in covered boxes

[image: ][image: ]GFCIs where required & operable

[image: ][image: ]Switches, outlets & fixtures operable

[image: ][image: ]Minimum 2 spaced outlets in all rooms

[image: ][image: ]Adequate light fixtures, with globes as needed

[image: ][image: ]Buffer space around lights to combustibles

[image: ][image: ]Safe, limited use of extension cords

[image: ]Exterior lines secure & protected [image: ][image: ]All installations maintained to code

__________________________________
__________________________________
__________________________________
Water Heater:
[image: ][image: ]Gas shut-off valve

[image: ][image: ]Proper pop-off valve & drop pipe

[image: ][image: ]Vent secured & properly pitched

[image: ]Operable, with no rust holes or leaks [image: ][image: ]Adequate surrounding clearance

__________________________________
__________________________________
__________________________________
HVAC:
[image: ][image: ]Gas shut-off valve and on/off switch

[image: ][image: ]Vent secured & properly pitched

[image: ][image: ]Filters are cleaned periodically

[image: ][image: ]Operable, provides minimum 68 degrees

[image: ][image: ]Adequate surrounding clearance

[image: ][image: ]All equipment installed and maintained to code

__________________________________

__________________________________
__________________________________


Laundry:


[image: ]Proper dryer vent to exterior with cover [image: ][image: ]Gas shut-off valve, capped if unused

__________________________________
__________________________________

__________________________________
Sinks, Bathtubs & Showers:
[image: ][image: ]Operable, with hot & cold water

[image: ][image: ]Functioning drains with proper traps

[image: ][image: ]No leaks or drips

[image: ][image: ]Garbage disposal operable if present

__________________________________
__________________________________

__________________________________
Toilets:
[image: ][image: ]Operating properly

[image: ][image: ]No leaks or continuous running

__________________________________
__________________________________

__________________________________
General Plumbing:
[image: ][image: ]Installed correctly with no leaks

[image: ][image: ]Proper venting

[image: ][image: ]Functioning drains with proper traps & covers

__________________________________
__________________________________
__________________________________
Stairways:
[image: ][image: ]Handrails if 4 or more steps

[image: ][image: ]Lighted correctly

[image: ][image: ]Steps stable, unbroken & of adequate strength

________________________________________

Windows:

[image: ][image: ]Proper locations & sizes for light & ventilation

[image: ][image: ]Proper for egress and lockable

[image: ][image: ]Snug fit, operable & not broken or cracked

[image: ]Bathrooms need mechanical or window venting [image: ][image: ]Screens are present & in good condition

_________________________________

__________________________________
__________________________________


[bookmark: page2]Smoke Detectors:

[image: ][image: ]Properly installed and operable [image: ][image: ]Installed in correct locations

[image: ][image: ]LR [image: ][image: ]DR[image: ][image: ] BD 1 [image: ][image: ]BD 2 [image: ][image: ]BD 3 [image: ]BD 4 [image: ][image: ]Other

__________________________________
__________________________________
__________________________________

Rooms

[image: ][image: ]Walls, floors & ceilings intact & maintained

[image: ][image: ]LR [image: ]DR[image: ] BD 1 [image: ]BD 2 [image: ]BD 3 [image: ]BD 4 [image: ]Other


[image: ][image: ]No padlocks or interior key locks on doors

[image: ][image: ]LR [image: ]DR[image: ] BD 1 [image: ]BD 2 [image: ]BD 3 [image: ]BD 4 [image: ]Other


[image: ][image: ]Unobstructed egress within and out of home

[image: ][image: ]LR [image: ]DR[image: ] BD 1 [image: ]BD 2 [image: ]BD 3 [image: ]BD 4 [image: ]Other


[image: ][image: ]Adequate area & height & proper layout

[image: ][image: ]LR [image: ]DR[image: ] BD 1 [image: ]BD 2 [image: ]BD 3 [image: ]BD 4 [image: ]Other


[image: ][image: ]Fireplaces, wood stoves operable & maintained

[image: ][image: ]LR [image: ]DR[image: ] BD 1 [image: ]BD 2 [image: ]BD 3 [image: ]BD 4 [image: ]Other


[image: ][image: ]No rubbish or garbage accumulation

[image: ][image: ]LR [image: ]DR[image: ] BD 1 [image: ]BD 2 [image: ]BD 3 [image: ]BD 4 [image: ]Other


[image: ]Basement bedrooms/rooms have egress windows

[image: ][image: ]LR [image: ][image: ]DR[image: ][image: ] BD 1 [image: ][image: ]BD 2 [image: ][image: ]BD 3 [image: ][image: ]BD 4 [image: ][image: ]Other


[image: ][image: ]Bedrooms and bathrooms have privacy doors

[image: ][image: ]BA1 [image: ][image: ]BA2 [image: ][image: ] BD1 [image: ][image: ]BD2 [image: ][image: ]BD3 [image: ][image: ]BD4


[image: ] Closet lights away from combustibles, up to code and operable

[image: ][image: ] BD 1 [image: ][image: ]BD 2 [image: ]BD 3 [image: ]BD 4 [image: ][image: ]Other


[image: ][image: ]Kitchen floors in good condition

__________________________________
__________________________________

__________________________________
__________________________________
__________________________________

__________________________________

Exterior Doors:

[image: ][image: ]Proper for egress and lockable

[image: ][image: ]Snug fit, operable & unbroken

_________________________________

__________________________________
__________________________________

Building Exterior:

[image: ][image: ]Roof waterproof & maintained

[image: ][image: ]Walls, foundations, chimney maintained

[image: ][image: ]Porches solid & maintained

[image: ]Guardrails on porches over 30” high [image: ][image: ]Handrails if 4 or more steps

__________________________________
__________________________________

__________________________________

Yard:

[image: ][image: ]Grass, shrubs, trees maintained to code

[image: ][image: ]Accessory structures maintained to code

[image: ][image: ]No illegal vehicles or illegal parking

[image: ][image: ]No rubbish or garbage

[image: ][image: ]Have garbage containers with covers

__________________________________
__________________________________
__________________________________




This is a checklist of common violations of the West Lafayette Housing-Property Maintenance Code (BOCA, 1978) as adopted by Ordinance 20-78 (Chapter 112, West Lafayette City Code). This checklist is not a comprehensive list of all code provisions and requirements applicable in the City of West Lafayette.
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