[bookmark: page1][image: ]Borough of North East Rental Inspection Program Checklist
[image: ]

Exterior Property Checklist

Chimneys
· Mortar joints

· Missing brick(s)

Roofs
· Damaged / in disrepair
· Notes


Gutters/Downspouts
· Missing gutters and/or downspouts
· Gutters / downspouts need repair

Exterior Walls /Trim
· Walls need repair
· Broken trim/corner boards
· Deteriorated/rotten siding
· Deteriorated soffit and/or fascia boards
· Loose and/or peeling paint
· Notes


Foundation Walls
· Mortar joints loose/deteriorating
· Repairs needed
· Notes


Steps, Handrails/Guards
· Broken/missing steps
· Missing handrails/guardrails
· Poor condition/not firmly fastened

· Notes


Windows & Doors / Frames and Trim
· Repair window frames
· Provide screens
· Broken/cracked glass
· Deteriorated frame/sash
· Missing glass
· Doors and frames not maintained
· Missing/broken knobs

· Inadequate locks

Exterior Yard Areas
· Accumulation of rubbish and garbage
· Overgrown weeds or grass
· Unregistered or junk vehicles
· Notes
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Interior Property Checklist


Living Room and/or Dining Room

· Defective/missing smoke detector
· Insufficient electrical outlets
· Defective windows

· Defective walls
· Defective ceilings
· Defective floors

· Hazardous use of electrical extension cords

· Missing/ damaged outlet covers
· Defective windows/hardware
· Defective doors/hardware
· Defective floors

· Defective walls
· Defective ceilings
· Notes


Kitchen
· Defective sink/faucet

· Defective drains
· Insufficient water pressure
· Kitchen cabinetry defective
· Defective floors
· Defective ceiling

· Defective walls
· Insufficient electric outlets

· Hazardous use of electrical extension cords

· Insects/vermin present
· Notes


Bathroom
· Defective toilet
· Defective bathtub/shower

· Inadequate ventilation

· Defective drains
· Electrical hazards
· GFCI needed
· Defective floor
· Defective walls
· Defective ceiling

· Privacy door needed
· Notes


Bedrooms
· Defective/missing smoke detector(s)
· Insufficient electrical outlets



· Defective windows
· Defective walls
· Defective ceilings
· Defective floors

· Hazardous use of electrical extension cords

· Area too small (min 70 sq.ft.)

· Notes




Bedrooms
· Defective/missing smoke detector(s)

· Insufficient electrical outlets
· Defective windows
· Defective walls

· Defective ceilings
· Defective floors

· Hazardous use of electrical extension cords

· Area too small (min 70 sq.ft.)
· Notes




Bedrooms
· Defective/missing smoke detector(s)

· Insufficient electrical outlets
· Defective windows
· Defective walls
· Defective ceilings

· Defective floors

· Hazardous use of electrical extension cords

· Area too small (min 70 sq.ft.)
· Notes
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Interior Property Checklist -Continued




Basement
· Improper gas shut-off valve
· Defective flue pipe

· Flue not mortared to chimney properly
· Improper water heater connection

· Hot water tank discharge pipe needed

· Uninspected electrical service panel
· Improper wiring
· Exposed wiring/boxes
· Improper use of 30 amp fuses

· Washing machine safe-waste needed
· Improper drains
· Improper stairs and/or handrails
· Smoke detectors absent
· Illegal basement sleeping rooms
· Foundation repairs needed
· Broken basement windows

· Unsanitary condition present (sewage)

· Basement Unsanitary (garbage, junk etc.)
· Insects and/or vermin present
· Notes


Attic
· Insufficient handrails/guards

· Defective steps
· Absent smoke detector
· Exposed wiring/boxes
· Roof leaks

· Unsanitary or Fire Hazard (accumulation of debris)
· Broken windows

· Note _______________________





Zoning

· Property not in compliance with zoning regulations
· Follow up required
· Notes


Fire and Life Safety Issues
· Means of Egress issues
· Smoke detectors

· Notes










3

[bookmark: page4][image: ]Borough of North East Rental Inspection Program Checklist
[image: ]
































































4
image1.jpeg




image2.png




